**G13 LED TUBELIGHTS**

**ITEM NO: VT-6272 SMD; WATTS: 10W**

|  |  |
| --- | --- |
| Item No: | VT-6272 SMD |
| SKU Code | **6144:6000K** |
| Type | **T8** |
| Base | **G13** |
| Real Watts | **10W** |
| EQ. Watts | **18W** |
| Voltage | **220~240V** |
| Input Frequency | **50Hz** |
| Input Efficiency | **80lm/w** |
| Lumen(lm) | **800lm** |
| PF | **>0.5** |
| CRI | **>80** |
| Color Temperature | **3000K,4500K,6000K** |
| Beam Angle | **240’D** |
| LED Chip | **SMD** |
| Protection Class | **IP20** |
| Body Material | **Glass** |
| Dimmable | **No** |
| Unit size | **600mmx28mm**  |
| Life Time | **20000hrs** |
| Operation Temperature | **-25 ~50’C** |
| Applicable Environment | **Indoor Lighting, Used in Home down light, Stairwell lighting.** |

 