
**LED BULBS**

**ITEM NO: VT-1929; WATTS:10W**

|  |  |
| --- | --- |
| Item No: | VT-1929 |
| SKU Codes | **4299:6000K** |
| Base | **E27** |
| Real Watts | **10W** |
| EQ. Watts | **100W** |
| Voltage | **200~240V** |
| Input Frequency | **50Hz** |
| Input Current | **50ma** |
| Input Efficiency | **85lm/w** |
| Lumen(lm) | **850lm** |
| PF | **>0.6** |
| RA | **>80** |
| Color Temperature | **4500K,6000K** |
| Beam Angle | **120’D** |
| LED Chip | **EPISTAR** |
| LED Type | **SMD** |
| LED Qty | **48** |
| Protection Class | **IP20** |
| Body Material | **Plastic** |
| Color of Fixture | **Powder Coating White ( PKW )** |
| Dimmable | **No** |
| Unit size | **180mm\*38mm** |
| Life Time | **20000hrs** |
| Operation Temperature | **-25 ~50’C** |
| Applicable Environment | **Indoor Lighting, Used in Home down light, Stairwell lighting.** |